# Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Period:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Grade: \_\_\_\_\_\_\_\_\_\_\_/200 points

## How to Properly Glue Wood

Use <https://nickcornwell.weebly.com/howtoproperlygluewood.html> to answer the following questions.

1. What needs to be done to your lumber before you glue?
2. What types of clamps do you use for edge gluing panels? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
3. Draw the grain direction of what a panel should look like that is made up of several pieces of lumber.
4. What is a dry clamp or a dry fit? Why do we do this?
5. What should we do if there are gaps when you dry fit your panel?
6. What is a cabinetmaker’s V and why is it used? Draw an example and explain why it is used?
7. You remove excess glue from a glue up before it dries. True or False?
8. How do you find hidden glue after you have wiped the surface clean?
9. How do you make your own matching wood putty?
10. How and why do you use clamping pads?
11. What are clamping triangles? Why do you use them?
12. (50 points) On the top part of the back of this sheet, list the steps to glue up a segmented turning blank. Draw examples to show how this is done.
13. (50 points) On the bottom part of the back of this sheet, list the steps to glue up a laminated turning blank. Draw examples to show how this is done.