# Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Block:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Grade: \_\_\_\_\_\_\_\_\_\_\_/300 points

## Board Feet Terminology

**Instructions: In the left column, define the term. In the right column, copy and paste a photo that illustrates the definition. Use** <https://nickcornwell.weebly.com/typesofwoodjoints.html>

|  |  |  |
| --- | --- | --- |
| 1. Board Feet-
 |  |  |
| 1. Linear Feet-
 |  |  |
| 1. Riftsawn lumber
 |  |  |
| 1. Flatsawn lumber
 |  |  |
| 1. Quarter sawn lumber
 |  |  |
| 1. FAS- First and Seconds
 |  |  |
| 1. F1F/ FAS One face-
 |  |  |
| 1. SEL- Select
 |  |  |
| 1. 1C/ No. 1 Common-
 |  |  |
| 1. Kiln-dried lumber-
 |  |  |
| 1. Air-dried lumber
 |  | **Show a photo of a lumber stack that is sticked to dry.** |
| 1. S1S- surface one side
 |  |  |
| 1. S2S- surface two sides
 |  |  |
| 1. S4S- surface four sides
 |  |  |
| 1. Rough cut lumber
 |  |  |